EGNSS4CAP CRON SCRIPT SOURCE CODE OVERVIEW

Below is a technical overview of the implemented cron script and its features.

**https://installation-server.tld/ws/cron\_locate\_by\_info.php**

* executed every 5 minutes
* computes photo location by network cell ID

**https://installation-server.tld/ws/cron\_check\_location.php**

* executed every 5 minutes
* compares locations from GNSS and by network cell ID, marks photo position as valid/invalid